The Default Modules

About System Module
This page shows a brief summary about your system, your distribution, KDE Plasma Version, KDE Frameworks Version, Qt Version, Kernel Version and OS Type; and in the hardware section information about Processors and Memory.
Use the information on this page if you ask for help in support channels or report a bug at 's bugtracker.

Memory Information Module
This module displays the current memory usage. It is updated constantly, and can be very useful for pinpointing bottlenecks when certain applications are executed.

Memory Types
The first thing you must understand, is there are two types of memory, available to the operating system and the programs that run within it.
The first type, is called physical memory. This is the memory located within the memory chips, within your computer. This is the RAM (for Random Access Memory) you bought when you purchased your computer.
The second type of memory, is called virtual or swap memory. This block of memory, is actually space on the hard drive. The operating system reserves a space on the hard drive for swap space. The operating system can use this virtual memory (or swap space), if it runs out of physical memory. The reason this is called swap memory, is the operating system takes some data that it doesn't think you will want for a while, and saves that to disk in this reserved space. The operating system then loads the new data you need right now. It has swapped the not needed data, for the data you need right now. Virtual or swap memory is not as fast as physical memory, so operating systems try to keep data (especially often used data), in the physical memory.
The total memory, is the combined total of physical memory and virtual memory.

Memory Information Module
This window is divided into a top and bottom section
The top section shows you the total physical memory, total free physical memory, shared memory, and buffered memory.
All four values are represented as the total number of bytes, and as the number of megabytes (1 megabyte = slightly more than 1,000,000 bytes)
The bottom section shows you three graphs:
Total Memory (this is the combination of physical and virtual memory).
Physical Memory
Virtual memory, or Swap Space.
The grey areas are free, and the blue and green areas are used.
The exact values of each type of memory are not critical, and they change regularly. When you evaluate this page, look at trends.
Does your computer have plenty of free space (grey areas)? If not, you can increase the swap size or increase the physical memory.
Also, if your computer seems sluggish: is your physical memory full, and does the hard drive always seem to be running? This suggests that you do not have enough physical memory, and your computer is relying on the slower virtual memory for commonly used data. Increasing your physical memory will improve the responsiveness of your computer.

Energy Information Module
This provides information about CPU wakeups, battery percentage and consumption over a user defined history and detailed information about the battery.

File Indexer Monitor Module
This Module shows the state of the file indexer. If the indexer is not running you can start it and then suspend or resume the indexing.

Device Information Module
Device Information is a device viewer module. It shows all relevant devices that are present within your PC. It has three sections, a device viewer, a information panel and a UDI listing for the currently selected device.

Device Viewer
The device viewer displays all the current devices detected on your PC in a tree. The main topics at the beginning of the tree are the device categories, left click on a collapsed category to expand it and vice versa to collapse it. To display information about a device, left click on the device in the viewer, the information will display on the right side information panel. You can right click on the device viewer to show the following options:
Collapse All: Collapses the tree to show only the main categories.
Expand All: Expands the tree to show all the children devices.
Show All Devices: Show all the categories no matter if devices are present in those categories
Show Relevant Devices: Only show categories that have devices present.
The default display is to collapse all while showing only relevant devices. Please note that the devices shown in the device listing are not all devices within your PC, they are just devices that have been detected via the Solid.
The device viewer can show the following devices:
Processors: These are your computers CPUs ( Central Processing Units ).
Storage Drives: Devices that are used to store your PCs files and data.
Network Interfaces: Devices that allow you to connect to a network or to another PC.
Audio Interfaces: Devices that allow your PC to play Sound. They are split into 2 categories, ALSA and OSS sound architectures.
Video Devices: Devices that allow you to stream live video.
Serial Devices: Devices that are connected to your serial port in your PC.
Smart Card Devices: Devices that are smart card readers.
Digital Video Broadcasting Devices: Devices that use the open standards for digital television.
Device Buttons: These are buttons that are present on your PC or external devices.
Batteries: These are battery devices that are plugged into your laptop.
AC Adapters: These devices will be present when you plug in your AC Adapter.
Multimedia Players: Devices that play media files, like a music player.
Camera Devices: These are digital camera that are connected to your PC.
Video devices do not include your video card adapter

Information Panel
The information panel is where device information is shown when you select a device. The first two information topics are always:
Product: The name of the device.
Vendor: The vendors name of the device.
The following information topics are dependent on the device chosen. They are labeled with easy to understand names. The information labels have the ability to be selected and copied from.
Processor Max Speed and Supported Instruction sets topics are usual not set by solid.
Top categories in the device listing do not show any information.

UDI Information
The bottom information panel shows the current selected devices UDI. This is the unique device identifier.
All labels have the ability to be selected and copied from.

Interrupt Request (IRQ) Information Module
This page displays information about the Interrupt Request Lines in use, and the devices that use them.
An IRQ is a hardware line used in a PC by (ISA bus) devices like keyboards, modems, sound cards, , to send interrupt signals to the processor to tell it that the device is ready to send or accept data. Unfortunately, there are only sixteen IRQ's (0-15) available in the i386 (PC) architecture for sharing among the various ISA devices.
Many hardware problems are the result of IRQ conflicts, when two devices try to use the same IRQ, or software is misconfigured to use a different IRQ from the one a device is actually configured for.
The exact information displayed is system-dependent. On some systems, IRQ information cannot be displayed yet.
On , this information is read from /proc/interrupts, which is only available if the /proc pseudo-filesystem is compiled into the kernel.
The first column, is the IRQ number. The second column, is the number of interrupts that have been received since the last reboot. The third column shows the type of interrupt. The fourth, identifies the device assigned to that interrupt.
The user cannot modify any settings on this page.

DMA Channel Information Module
This page displays information about the DMA (Direct Memory Access) Channels. A DMA channel is a direct connection that allows devices to transfer data to and from memory without going through the processor. Typically, i386-architecture systems (PC's) have eight DMA channels (0-7).
The exact information displayed is system-dependent. On some systems, DMA Channel information cannot be displayed yet.
On , this information is read from /proc/dma, which is only available if the /proc pseudo-filesystem is compiled into the kernel.
A list of all currently-registered (ISA bus) DMA channels that are in use is shown. The first column shows the DMA channel, and the second column shows the device which uses that channel.
Unused DMA channels are not listed.
The user cannot modify any settings on this page.

IEEE 1394 Device Information Module
The IEEE 1394 interface, also known as FireWire, is a serial bus interface standard for high-speed communications and isochronous real-time data transfer.
The list in this module displays all devices attached to IEEE 1394 bus and allows you to reset the bus by clicking the Generate 1394 Bus Reset button.
The meaning of the columns in this list:
Name: port or node name, the number can change with each bus reset
GUID: the 64 bit GUID of the node
Local: checked if the node is an IEEE 1394 port of your computer
IRM: checked if the node is isochronous resource manager capable
CRM: checked if the node is cycle master capable
ISO: checked if the node supports isochronous transfers
BM: checked if the node is bus manager capable
PM: checked if the node is power management capable
Acc: the cycle clock accuracy of the node, valid from 0 to 100
Speed: the speed of the node
Vendor: the vendor of the device

USB Controller/USB Devices Information Module
This module allows you to see the devices attached to your USB bus(es).
This module is for information only, you cannot edit any information you see here.

Input/Output Port Information Module
This page displays information about the I/O ports.
I/O Ports are memory addresses used by the processor for direct communication with a device that has sent an interrupt signal to the processor.
The exchange of commands or data between the processor and the device takes place through the I/O port address of the device, which is a hexadecimal number. No two devices can share the same I/O port. Many devices use multiple I/O port addresses, which are expressed as a range of hexadecimal numbers.
The exact information displayed is system-dependent. On some systems, I/O port information can not yet be displayed.
On , this information is read from /proc/ioports which is only available if the /proc pseudo-filesystem is compiled into the kernel. A list of all currently-registered I/O port regions that are in use is shown.
The first column is the I/O port (or the range of I/O ports), the second column identifies the device that uses these I/O ports.
The user cannot modify any settings on this page.

PCI-bus/Installed PCI Cards Information Module
This page displays information about the PCI-bus and installed PCI cards, and other devices that use the Peripheral Component Interconnect (PCI) bus.
The exact information displayed is system-dependent. On some systems, PCI-information can not yet be displayed.
On , this information is read from /proc/pci which is only available if the /proc pseudo-filesystem is compiled into the kernel. A listing of all PCI devices found during kernel initialization, and their configuration, is shown.
Each entry begins with a bus, device and function number.
The user cannot modify any settings on this page.

Network Information Module

Network Interfaces Information Module
This page displays information about the network interfaces installed in your computer.
The exact information displayed is system-dependent. On some systems, this information can not yet be displayed.
The user cannot modify any settings on this page.

Samba Status Information Module
The Samba and NFS Status Monitor is a front end to the programs smbstatus and showmount. Smbstatus reports on current Samba connections, and is part of the suite of Samba tools, which implements the SMB (Server Message Block) protocol, also called the NetBIOS or LanManager protocol.
This protocol can be used to provide printer sharing or drive sharing services on a network including machines running the various flavors of .
showmount is part of the NFS software package. NFS stands for Network File System and is the traditional way to share folders over the network. In this case the output of showmount -a localhost is parsed. On some systems showmount is in /usr/sbin, check if you have showmount in your PATH.

Exports
On this page you can see a big list which shows the currently active connections to Samba shares and NFS exports of your machine. The first column shows you whether the resource is a Samba (SMB) share or a NFS export. The second column contains the name of the share, the third the name of the remote host, which accesses this share. The remaining columns have only a meaning for Samba-shares.
The fourth column contains the User ID of the user, who accesses this share. Note that this does not have to be equal to the user ID of this user. The same applies for the next column, which displays the group ID of the user.
Each connection to one of your shares is handled by a single process (smbd), the next column shows the process ID (pid) of this smbd. If you kill this process the connected user will be disconnected. If the remote user works from , as soon as this process is killed a new one will be created, so he will almost not notice it.
The last column shows how many files this user has currently open. Here you see only, how many files he has open just now, you don't see how many he copied or formerly opened

Imports
Here you see which Samba- and NFS-shares from other hosts are mounted on your local system. The first column shows whether it is a Samba- or NFS-share, the second column displays the name of the share, and the third shows where it is mounted.
The mounted NFS-shares you should see on (this has been tested), and it should also work on (this has not been tested).

Log
This page presents the contents of your local samba log file in a nice way. If you open this page, the list will be empty. You have to press the Update button, then the samba log file will be read and the results displayed. Check whether the samba log file on your system is really at the location as specified in the input line. If it is somewhere else or if it has another name, correct it. After changing the file name you have to press Update again.
Samba logs its actions according to the log level (see smb.conf). If loglevel = 1, samba logs only when somebody connects to your machine and when this connection is closed again. If log level = 2, it logs also if somebody opens a file and if he closes the file again. If the log level is higher than 2, yet more stuff is logged.
If you are interested in who accesses your machine, and which files are accessed, you should set the log level to 2 and regularly create a new samba log file (⪚ set up a cron task which once a week moves your current samba log file into another folder or something like that). Otherwise your samba log file may become very big.
With the four checkboxes below the big list you can decide, which events are displayed in the list. You have to press Update to see the results. If the log level of your samba is too low, you won't see everything.
By clicking on the header of one column you can sort the list by this column.

Statistics
On this page you can filter the contents of the third page for certain contents.
Let's say the Event field (not the one in the list) is set to Connection, Service/File is set to *, Host/User is set to *, Show expanded service info is disabled and Show expanded host info is disabled.
If you press Update now, you will see how often a connection was opened to share * ( to any share) from host * ( from any host). Now enable Show expanded host info and press Update again. Now you will see for every host which matches the wildcard *, how many connections were opened by him.
Now press Clear Results.
Now set the Event field to File Access and enable Show expanded service info and press Update again.
Now you will see how often every single file was accessed. If you enable Show expanded host info too, you will see how often every single user opened each file.
In the input lines Service/File and Host/User you can use the wildcards * and ? in the same way you use them at the command line. Regular expressions are not recognized.
By clicking on the header of a column you can sort the list by this column. This way you can check out which file was opened most often, or which user opened the most files or whatever.

Section Author
Module copyright 2000: Michael Glauche and
Originally written by: Michael Glauche
Currently maintained by:

Contributors
Conversion to kcontrol applet:
Use of K3Process instead of popen, and more error checking:
Conversion to kcmodule, added tab pages 2,3,4, bug fixed:
Documentation copyright 2000
Documentation translated to docbook by

Graphical Information Module
When you open the modules in this section, you are presented with some information. The left hand side of the window is organized into a tree. Some of the elements have a plus sign in front of the label. Clicking this sign opens a submenu related to the label. Clicking on a minus sign in front of a label hides the submenu.
The right hand side of the window contains the individual values for each of the parameters on the left.
The information presented will vary depending on your setup.
Some setups may not be able to determine some or all of the parameters.
You can not change any values from this module. It is for information only.

Wayland Information Module
This screen is useful for getting specific information about your Wayland Compositor.

X Server Information Module
This screen is useful for getting specific information about your X Server and the current session of X.

OpenGL Information Module
This page displays information about installed OpenGL implementation. OpenGL (for "Open Graphics Library") is a cross-platform, hardware independent interface for 3D graphics.
GLX is the binding for OpenGL to X Window system.
DRI (Direct Rendering Infrastucture) provides hardware acceleration for OpenGL. You must have a videocard with 3D accelerator and properly installed driver for this.
Read more at the official OpenGL site OpenGL